G.V.K. IBES Co. Inc. P.O. Box 536 Webster, Ma. 01570 
www.enviro-earth.comlemail: greggvk@gmail.comtel/fax: 1-508-949-0939 cell: 1-774-253-1776 
MATERIAL SAFETY DATA SHEET 
Section 1 - Identification 
Product Name: 
VIC-Graffiti Remover - Painted Surfaces 
VIC- Graffiti Remover - Unpainted Surfaces 
VIC- Ultimate Graffiti Remover 
VIC- Graffiti Wipes 
Soy-Based Mixture 
Trade Secret 
Trade Secret 
Chemical Name: 
Chemical Family: 
Chemical 
Fonnula: 
HMIS: 
Health: 
Flammability: 
Physical 
Hazard: 
PPE: 
Section 1 1 - Composition Infonnation on Ingredient 
Trade Secret - Specific chemical identities will be made available to 
medical professionals and others as required by 29 CFR 1910.1200 (i) (iv) 
1 
1 
o 
B 
NFPA 
Health: 
Flammability: 
Reactivity: 
Special Hazard: 
1 
1 
o 
Non 
e 
Vic-Graffiti Remover - Unpainted Surfaces (only) 
Composition: 	N-Methyl-2-Pyrrolidone 	Weight 
OSHA TWA: NK 	ACGIH TLV:M 	CAS Number: 
<20% 
872-50- 
4 
Ultimate Graffiti Remover (only) 
Composition: 	N-MethYI-2-pyrrolidone 	Weight: 
OSHA TWA NK 	ACGIH TLV:M 	CAS Number: 
<40% 
872-50- 
4 
Section III - Hazards Identification 
Health Hazards (Acute and Chronic): 
Acute: 	May cause eye irritation. May cause abdominal 
discomfort, nausea, and diarrhea if swallowed. 
Chronic: 	iIIo known adverse effects. 
Medical Conditions Generally Aggravated by Exposure: None known 
Section IV - First Aid Measures 
Inhalation: 	Remove to fresh air, 
Skin: 	Wash thoroughly with soap and water. Remove 
soiled clothing and wash before reuse. 
Get medical attention. 
DO NOT RUB EYES. Immediately Hush 
thoroughly with plenty of water. Get medical 
atlention. If discomfort or symptoms develop, get 
medical atlention. 
Ingestion
Eyes: 
Section V - Fire and Explosion Hazard Data 
Flash Point (Method Used): 	> 200°F- Open Cup 
Flammable Limits: 	Not determined 
Extinguishing Media: 	Water spray, dry chemical, foam 
and CO2, 
Fire Fighting Procedures: 	Treat as oil fire. Use water spray 
to cool fire-exposed containers. 
Fire and Explosion Hazards: Rags soaked with any solvent present a 
fire hazard and should always be stored in UL listed 
or Factory Mutual approved, covered containers. 
Improperly stored rags can create conditions that lead 
to spontaneous combustion. This product contains 
antioxidants to retard oxidation. 
Section VI - Accidental Release Measures 
Avoid uncontrolled releases of this material into the environment Contain 
spilled material. Where necessary, collect using absorbent media. Transfer 
to secure labelled containers. 
Section VII- Precautions for Safe Handling and Use 
Precautions to be taken in handling and storing: 
Store upright in a cool, dry well ventilated area, in tightly closed containers 
away from combustible materials, material used in combination with any 
other materials or in any other applications. The stated MSDS is reliable 
to the best of the company's knowledge and believed accurate as of the 
date indicated. 
Section VIII - Exposure Controls/Personal Protection 
Ventilation/Engineering Controls: 
Respiratory protection: 
Adequate general ventilation 
None required where adequate 
ventilation conditions exist 
Chemical splash goggles 
recommended. 
Impervious gloves 
recommended. 
Wear suitable clothing to avoid 
skin contact 
Do not smoke in areas of 
storage 
or use. Avoid contact with eyes. 
Wash with soap and water 
immediately after handling. 
Section IX - Physical and Chemical Characteristics 
Boiling Point: 	> 483°F 
Solubility in Water: 	Partially soluble 
Specific Gravity (HP = 1): 	0.963 - 0.975 
Melting Point: 	30°F 
Appearance: 	GR-P, GR-UP, and UGR 
Light Brown Viscous liquid 
GR Wipes - Light Yellow Liquid 
Mild 
Eye protection: 
Skin protection: 
Other protective clothing 
or equipment: 
Work/Hygienic practices: 
Odor: 
Section X - Stability and Reactivity 
Stability: 
Conditions to Avoid: 
Incompatibility (Materials to Avoid): 
Hazardous Decomposition Byproducts: 
Hazardous Polymerization: 
Stable 
Excessive heat or open flame. 
Strong oxidizing agents. Acids 
CO and CO2 may be produced. 
Will not occur. 
Section XI - Toxiiogical Infonnation 
Eye irritant This product does not contain any ingredient designated by 
IARC, 
NTP, ACGIH or OSHA as a probable or suspected human carcinogens. 
Section XII- Ecological Infonnation 
Aquatic toxicity rating not determined. All possible measures should be 
taken to prevent release into the environment 
Section XIII- Disposal Considerations. 
Disposal of all product and used clean up materials must be in accordance 
with all applicable federal, state and local regulations. 
Section XIV - Transport Information 
Not requiated. 
Section XV - Regulatory Infonnation 
U.S. FEDERAL REGULATIONS: 
TOXIC SUBSTANCES CONTROL ACT (TSCA) 
All components are included in the EPA Toxic Substance Control Act 
(TSCA) 
Chemical Substance Inventory. 
OSHA Hazard Communication Standard (29CFR1910.1200) hazard 
class(es): 	Eye Irritant 
STATE REGULATIONS: 
State of Califomia Safe Drinking Water and Toxic Enforcement Act of 1986 
(Proposition 65): Graffiti Remover-Unpainted Surfaces (only) contains one 
or more chemicals known to cause reproductive toxcicity_ 
Consult the regulations of the given state. 
INTERNATIONAL REGULATIONS: 
Consult the regulations of the importing country. 
Section XVI- Other Information 
MSDS is reliable to the best of the company's knowledge. For detailed 
MSDS, contact company at 1-774-253-1776 or greggvk@gamil.com